{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["CMT2300A"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CMT2300A","index":0,"n_rows":123,"n_cols":13,"rows_kept":123,"merged":[[2,0,3,0],[2,4,13,11],[2,12,13,12],[4,0,5,0],[6,0,7,0],[8,0,9,0],[10,0,11,0],[12,0,14,0],[15,0,16,0],[15,4,15,5],[15,6,15,7],[15,8,15,9],[15,10,15,11],[15,12,26,12],[17,0,18,0],[17,5,17,7],[17,8,17,9],[17,10,17,11],[18,4,18,11],[19,0,20,0],[19,5,19,7],[19,8,19,11],[20,4,20,11],[21,0,22,0],[21,5,21,7],[21,8,21,11],[22,4,22,11],[23,0,24,0],[23,5,23,7],[23,8,23,11],[24,8,24,11],[25,0,26,0],[25,5,25,6],[25,7,25,8],[25,9,25,11],[26,4,26,5],[26,7,26,11],[28,0,29,0],[28,4,35,11],[28,12,35,12],[30,0,31,0],[32,0,33,0],[34,0,35,0],[37,0,38,0],[37,4,60,11],[37,12,60,12],[39,0,40,0],[41,0,42,0],[43,0,44,0],[45,0,46,0],[47,0,48,0],[49,0,50,0],[51,0,52,0],[53,0,54,0],[55,0,56,0],[57,0,58,0],[59,0,60,0],[62,0,63,0],[62,4,62,8],[62,10,62,11],[62,12,90,12],[63,4,63,11],[64,0,65,0],[64,4,64,11],[65,4,65,11],[66,0,67,0],[66,5,66,7],[66,8,66,10],[67,4,67,11],[68,0,69,0],[68,4,68,11],[69,4,69,11],[70,0,71,0],[70,4,70,11],[71,4,71,11],[72,0,73,0],[72,4,72,11],[73,4,73,11],[74,0,75,0],[74,4,74,11],[75,5,75,7],[76,0,77,0],[76,4,76,11],[77,8,77,9],[77,10,77,11],[78,0,79,0],[78,4,78,11],[79,4,79,11],[80,0,81,0],[80,4,80,11],[81,4,81,11],[82,0,83,0],[82,9,82,10],[83,4,83,11],[84,0,85,0],[84,4,84,11],[85,7,85,8],[86,0,87,0],[86,4,86,11],[87,10,87,11],[88,0,89,0],[88,4,88,11],[89,4,89,11],[90,0,92,0],[90,5,90,11],[92,4,102,11],[92,12,102,12],[93,0,94,0],[95,0,96,0],[97,0,98,0],[99,0,100,0],[101,0,102,0],[104,4,104,11],[104,12,114,12],[105,8,105,11],[107,4,107,11],[108,4,108,11],[109,6,109,7],[109,8,109,9],[109,10,109,11],[110,7,110,11],[111,7,111,11],[113,5,113,6],[116,12,122,12],[120,4,120,11],[121,4,121,11],[122,4,122,11],[130,8,130,9]],"flags":["formulas_cached_only"]}
[]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x00","RW","CUS_CMT1","用户无须理解，直接用RFPDK生成导入",{"$nulls":7},"CMT区"]
[null,"0x01","RW","CUS_CMT2"]
[null,"0x02","RW","CUS_CMT3"]
[null,"0x03","RW","CUS_CMT4"]
[null,"0x04","RW","CUS_CMT5"]
[null,"0x05","RW","CUS_CMT6"]
[null,"0x06","RW","CUS_CMT7"]
[null,"0x07","RW","CUS_CMT8"]
[null,"0x08","RW","CUS_CMT9"]
[null,"0x09","RW","CUS_CMT10"]
[null,"0x0A","RW","CUS_CMT11"]
[null,"0x0B","RW","CUS_RSSI"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x0C","RW","CUS_SYS1","LMT_VTR [1:0]",null,"MIXER_BIAS [1:0]",null,"LNA_MODE [1:0]",null,"LNA_BIAS [1:0]",null,"系统区"]
[null,"0x0D","RW","CUS_SYS2","LFOSC_RECAL_EN","LFOSC_CAL1_EN","LFOSC_CAL2_EN","RX_TIMER_EN","SLEEP_TIMER_EN","TX_DC_EN","RX_DC_EN","DC_PAUSE"]
[null,"0x0E","RW","CUS_SYS3","SLEEP_BYPASS_EN","XTAL_STB_TIME [2:0]",null,null,"TX_EXIT_STATE [1:0]",null,"RX_EXIT_STATE [1:0]"]
[null,"0x0F","RW","CUS_SYS4","SLEEP_TIMER_M [7:0]"]
[null,"0x10","RW","CUS_SYS5",null,"SLEEP_TIMER_M [10:8]",null,null,"SLEEP_TIMER_R [3:0]"]
[null,"0x11","RW","CUS_SYS6","RX_TIMER_T1_M [7:0]"]
[null,"0x12","RW","CUS_SYS7",null,"RX_TIMER_T1_M [10:8]",null,null,"RX_TIMER_T1_R [3:0]"]
[null,"0x13","RW","CUS_SYS8","RX_TIMER_T2_M [7:0]"]
[null,"0x14","RW","CUS_SYS9",null,"RX_TIMER_T2_M [10:8]",null,null,"RX_TIMER_T2_R [3:0]"]
[null,"0x15","RW","CUS_SYS10","COL_DET_EN","COL_OFS_SEL","RX_AUTO_EXIT_DIS","DOUT_MUTE","RX_EXTEND_MODE [3:0]"]
[null,"0x16","RW","CUS_SYS11","PJD_TH_SEL","RSSI_VLD_SRC [1:0]",null,"RSSI_DET_SEL [1:0]",null,"RSSI_AVG_MODE [2:0]"]
[null,"0x17","RW","CUS_SYS12","PJD_WIN_SEL [1:0]",null,"RESV","RESV"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x18","RW","CUS_RF1","用户无须理解，直接用RFPDK生成导入",{"$nulls":7},"频率区"]
[null,"0x19","RW","CUS_RF2"]
[null,"0x1A","RW","CUS_RF3"]
[null,"0x1B","RW","CUS_RF4"]
[null,"0x1C","RW","CUS_RF5"]
[null,"0x1D","RW","CUS_RF6"]
[null,"0x1E","RW","CUS_RF7"]
[null,"0x1F","RW","CUS_RF8"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x20","RW","CUS_RF9","用户无须理解，直接用RFPDK生成导入",{"$nulls":7},"数据率区"]
[null,"0x21","RW","CUS_RF10"]
[null,"0x22","RW","CUS_RF11"]
[null,"0x23","RW","CUS_RF12"]
[null,"0x24","RW","CUS_FSK1"]
[null,"0x25","RW","CUS_FSK2"]
[null,"0x26","RW","CUS_FSK3"]
[null,"0x27","RW","CUS_FSK4"]
[null,"0x28","RW","CUS_FSK5"]
[null,"0x29","RW","CUS_FSK6"]
[null,"0x2A","RW","CUS_FSK7"]
[null,"0x2B","RW","CUS_CDR1"]
[null,"0x2C","RW","CUS_CDR2"]
[null,"0x2D","RW","CUS_CDR3"]
[null,"0x2E","RW","CUS_CDR4"]
[null,"0x2F","RW","CUS_AGC1"]
[null,"0x30","RW","CUS_AGC2"]
[null,"0x31","RW","CUS_AGC3"]
[null,"0x32","RW","CUS_AGC4"]
[null,"0x33","RW","CUS_OOK1"]
[null,"0x34","RW","CUS_OOK2"]
[null,"0x35","RW","CUS_OOK3"]
[null,"0x36","RW","CUS_OOK4"]
[null,"0x37","RW","CUS_OOK5"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x38","RW","CUS_PKT1","RX_PREAM_SIZE [4:0]",{"$nulls":4},"PREAM_LENG_UNIT","DATA_MODE [1:0]",null,"基带区"]
[null,"0x39","RW","CUS_PKT2","TX_PREAM_SIZE [7:0]"]
[null,"0x3A","RW","CUS_PKT3","TX_PREAM_SIZE [15:8]"]
[null,"0x3B","RW","CUS_PKT4","PREAM_VALUE [7:0]"]
[null,"0x3C","RW","CUS_PKT5","RESV","SYNC_TOL [2:0]",null,null,"SYNC_SIZE [2:0]",null,null,"SYNC_MAN_EN"]
[null,"0x3D","RW","CUS_PKT6","SYNC_VALUE [7:0]"]
[null,"0x3E","RW","CUS_PKT7","SYNC_VALUE [15:8]"]
[null,"0x3F","RW","CUS_PKT8","SYNC_VALUE [23:16]"]
[null,"0x40","RW","CUS_PKT9","SYNC_VALUE [31:24]"]
[null,"0x41","RW","CUS_PKT10","SYNC_VALUE [39:32]"]
[null,"0x42","RW","CUS_PKT11","SYNC_VALUE [47:40]"]
[null,"0x43","RW","CUS_PKT12"]
[null,"0x44","RW","CUS_PKT13","SYNC_VALUE [63:56]"]
[null,"0x45","RW","CUS_PKT14","RESV","PAYLOAD_LENG [10:8]",null,null,"AUTO_ACK_EN","NODE_LENG_POS_SEL","PAYLOAD_BIT_ORDER","PKT_TYPE"]
[null,"0x46","RW","CUS_PKT15","PAYLOAD_LENG [7:0]"]
[null,"0x47","RW","CUS_PKT16","RESV","RESV","NODE_FREE_EN","NODE_ERR_MASK","NODE_SIZE [1:0]",null,"NODE_DET_MODE [1:0]"]
[null,"0x48","RW","CUS_PKT17","NODE_VALUE [7:0]"]
[null,"0x49","RW","CUS_PKT18","NODE_VALUE [15:8]"]
[null,"0x4A","RW","CUS_PKT19","NODE_VALUE [23:16]"]
[null,"0x4B","RW","CUS_PKT20","NODE_VALUE [31:24]"]
[null,"0x4C","RW","CUS_PKT21","FEC_TYPE","FEC_EN","CRC_BYTE_SWAP","CRC_BIT_INV","CRC_RANGE","CRC_TYPE [1:0]",null,"CRC_EN"]
[null,"0x4D","RW","CUS_PKT22","CRC_SEED [7:0]"]
[null,"0x4E","RW","CUS_PKT23","CRC_SEED [15:8]"]
[null,"0x4F","RW","CUS_PKT24","CRC_BIT_ORDER","WHITEN_SEED [8]","WHITEN_SEED_TYPE","WHITEN_TYPE [1:0]",null,"WHITEN_EN","MANCH_TYPE","MANCH_EN"]
[null,"0x50","RW","CUS_PKT25","WHITEN_SEED [7:0]"]
[null,"0x51","RW","CUS_PKT26","RESV","RESV","RESV","RESV","RESV","RESV","TX_PREFIX_TYPE [1:0]"]
[null,"0x52","RW","CUS_PKT27","TX_PKT_NUM [7:0]"]
[null,"0x53","RW","CUS_PKT28","TX_PKT_GAP [7:0]"]
[null,"0x54","RW","CUS_PKT29","FIFO_AUTO_RES_EN","FIFO_TH [6:0]"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x55","RW","CUS_TX1","用户无须理解，直接用RFPDK生成导入",{"$nulls":7},"发射区"]
[null,"0x56","RW","CUS_TX2"]
[null,"0x57","RW","CUS_TX3"]
[null,"0x58","RW","CUS_TX4"]
[null,"0x59","RW","CUS_TX5"]
[null,"0x5A","RW","CUS_TX6"]
[null,"0x5B","RW","CUS_TX7"]
[null,"0x5C","RW","CUS_TX8"]
[null,"0x5D","RW","CUS_TX9"]
[null,"0x5E","RW","CUS_TX10"]
[null,"0x5F","RW","CUS_LBD"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x60","RW","CUS_MODE_CTL","CHIP_MODE_SWT [7:0]",{"$nulls":7},"控制区1  "]
[null,"0x61","RW","CUS_MODE_STA","RESV","RESV","RSTN_IN_EN","CFG_RETAIN","CHIP_MODE_STA [3:0]"]
[null,"0x62","RW","CUS_EN_CTL","RESV","RESV","UNLOCK_STOP_EN","LBD_STOP_EN","RESV","RESV","RESV","RESV"]
[null,"0x63","RW","CUS_FREQ_CHNL","FH_CHANNEL [7:0]"]
[null,"0x64","RW","CUS_FREQ_OFS","FH_OFFSET [7:0]"]
[null,"0x65","RW","CUS_IO_SEL","RESV","RESV","GPIO3_SEL [1:0]",null,"GPIO2_SEL [1:0]",null,"GPIO1_SEL [1:0]"]
[null,"0x66","RW","CUS_INT1_CTL","RF_SWT1_EN","RF_SWT2_EN","INT_POLAR","INT1_SEL [4:0]"]
[null,"0x67","RW","CUS_INT2_CTL","RESV","LFOSC_OUT_EN","TX_DIN_INV","INT2_SEL [4:0]"]
[null,"0x68","RW","CUS_INT_EN","SL_TMO_EN","RX_TMO_EN","TX_DONE_EN","PREAM_OK_EN","SYNC_OK_EN","NODE_OK_EN","CRC_OK_EN","PKT_DONE_EN"]
[null,"0x69","RW","CUS_FIFO_CTL","TX_DIN_EN","TX_DIN_SEL [1:0]",null,"FIFO_AUTO_CLR_DIS","FIFO_TX_RD_EN","FIFO_RX_TX_SEL","FIFO_MERGE_EN","SPI_FIFO_RD_WR_SEL"]
[null,"0x6A","W","CUS_INT_CLR1","RESV","RESV","SL_TMO_FLG","RX_TMO_FLG","TX_DONE_FLG","TX_DONE_CLR","SL_TMO_CLR","RX_TMO_CLR"]
[null,"Addr","R/W","Name","Bit 7","Bit 6","Bit 5","Bit 4","Bit 3","Bit 2","Bit 1","Bit 0","Function"]
[null,"0x6B","W","CUS_INT_CLR2","RESV","RESV","LBD_CLR","PREAM_OK_CLR","SYNC_OK_CLR","NODE_OK_CLR","CRC_OK_CLR","PKT_DONE_CLR","控制区2"]
[null,"0x6C","W","CUS_FIFO_CLR","RESV","RESV","RESV","RESV","RESV","FIFO_RESTORE","FIFO_CLR_RX","FIFO_CLR_TX"]
[null,"0x6D","R","CUS_INT_FLAG","LBD_FLG","COL_ERR_FLG","PKT_ERR_FLG","PREAM_OK_FLG","SYNC_OK_FLG","NODE_OK_FLG","CRC_OK_FLG","PKT_OK_FLG"]
[null,"0x6E","R","CUS_FIFO_FLAG","RESV","RX_FIFO_FULL_FLG","RX_FIFO_NMTY_FLG","RX_FIFO_TH_FLG","RX_FIFO_OVF_FLG","TX_FIFO_FULL_FLG","TX_FIFO_NMTY_FLG","TX_FIFO_TH_FLG"]
[null,"0x6F","R","CUS_RSSI_CODE","RSSI_CODE [7:0]"]
[null,"0x70","R","CUS_RSSI_DBM","RSSI_DBM [7:0]"]
[null,"0x71","R","CUS_LBD_RESULT","LBD_RESULT [7:0]"]